# VOLUME 3

# TECHNICAL SPECIFICATIONS

TECHNICAL SPECIFICATION

Renovation of a screening room that will house a fundus camera and 11 smaller medical devices-Reconstruction and equipping

total net area P = 43m2

PRIMARY WORKS

Dismantling of existing old built-in closets from plywood together with transport to the landfill up to 5 km in a place designated by the developer 1

Dismantling of existing old wall tiles with horizontal and vertical transport of the same to the landfill up to 5 km in a place determined by the developer m2 4,5

Dismantling of an existing old die with horizontal and vertical transport of the same to the landfill up to 5 km in a place determined by the investor pieces 1

Dismantling of existing old Venetian women with horizontal and vertical transport of the same to the landfill up to 5 km in a place determined by the investor 1

Disassembly of old lights and storage of the same in a place designated by the developer

pieces 4

TOTAL

OVERWHELMING WORKS

Procurement, transport and installation of PVC industrial floor with prior preparation of the substrate, partial patching of damaged parts and placement of an alma mater in three layers (final processing of the wall joint with the floor) m2 50

TOTAL

MOLEROFARBAR WORKS

All positions include mounting and demonizing the required scaffolding to perform the work

Paint the old ceilings with a dispersion paint with pre-patching, cracking of cracks and damaged parts m2 43

Painting old cracked walls with dispersion paint with pre-patching, cracking of cracks and damaged parts m2 35

Painting with matte greasy paint in a height of 1m from the floor in the color of your choice by the developer m2 12

Painting existing wooden doors with oily color in a tone of the investor's choice by pre-scraping and coating pieces 2

TOTAL

CERAMIC WORKS

wall tiles:

Purchase, transport and installation of GRES ceramic tiles (artificial granite), installation with tile adhesive laser cut without fugue, non-porous, frost-resistant, high temperatures, waterproof, wear-resistant, min 30 / 30cm

Complex with joined material, angular and finishing aluminum moldings m2 4,5

Purchase, transport and installation of a built-in sink with a width of 40 cm together with a siphon and a sitting faucet together with a water supply and drainage installation pieces 1

Purchase, transport and installation of a low-mounted boiler under the die. pieces 1

TOTAL

ELECTRICITY

Purchase, transport and installation of ceiling lights 60x60 with 4 neon lights with metal raster

pieces 4

TOTAL

EQUIPMENT

Making, transporting and assembling office desks with dimensions 80x140 of refined plywood e = 2.5cm, fitted with ABS tape together with a drawer pieces 2

Procurement and transport of ottoman - chair for examination with dimensions 190x60x56cm made of solid steel construction placed on four legs that can be used to regulate the chair to lie steadily on the substrate, the upper surface made of artificial leather pieces 2

Purchase and transport of a chair for examination made of steel profile with the possibility of vertical lifting and lowering depending on the need of the patients, a seat lined with artificial leather that is easy to maintain pieces 2

Purchase and transport of office chairs pieces 2

Purchase, transport and installation of a 70x100 desk designed for installing a Fundus camera

pieces 1

Purchase, transport and installation of ROLO curtains in color of the investor's choice

m2 18

Production, transport and installation of built-in closets made of refined plywood fitted with ABS tape with the following dimensions:

1) built-in closet 140х215х60 (WхHхL) pieces 2

2) built-in closet 140х60х60 (WхHхL) pieces 2

3) built-in closet 67x70x60 (WхHхL) pieces

4) built-in closet 67x215x60 (WхHхL) pieces 1

5) built-in closet 146х60х60 (WхHхL) pieces 1

6) built-in closet 125х60х60 (WхHхL) pieces 1

TOTAL

RECAPITULAR

PRIMARY WORKS

OVERWHELMING WORKS

MOLEROFARBAR WORKS

CERAMIC WORKS

ELECTRICITY

EQUIPMENT

Prices have to be without VAT !!!